Safe Work Procedure

**NOTE: DO NOT use this machine unless you have been trained in its safe use and operation.**

|  |  |
| --- | --- |
| Description of Work: | Using a High Pressure Water Cleaner  |
| High Pressure Water Cleaner   Description: 221015-thumb | **Potential Hazards:** Exposure to hazards associated with impact (from back spray), pressurised content, electricity, ergonomics, slips trips and falls and back spray containing water, dirt or debris. |
| **Personal Protective Equipment (PPE) Required** *(Check the box for required PPE*): |
| hand protectionGloves | dust maskFace Masks | safety gogglesEyeProtection | face shieldWelding Mask | foot protectionAppropriateFootwear | hearing protHearing Protection | safety apronProtective Clothing |
| [ ]  | [ ]  | [ ]  | [ ]  | [x]  | [ ]  | [ ]  |
|  **Safe Work Procedure Checklist:** |
| 1. PRE-Operation:* Check all parts and cords for any damage before use.
* Unwind high pressure hose fully from the hose drum.
* Use only attachments supplied and approved by the manufacturer.
* Wear appropriate PPE.

2. Operation:* The high pressure cleaner must not be directed at other people, animals or live electrical equipment.
* Ensure firm footing and hold the spray handgun and spray lance firmly in both hands whilst in operation.

3. POST-Operation:* Turn off appliance and press the lever to release any remaining pressure in the system.
* Disconnect the appliance from water supply
* Store the handgun and spray lance in the accessory point and store appropriately.
 |
| **Competent Persons** (The following persons are authorised to operate, supervise and test students on the equipment/process). |
| **Name:** | **Title:** | **Contact Details:** |
|  |  |  |
|  |  |  |