Safe Work Procedure

**NOTE: DO NOT use this machine unless you have been trained in its safe use and operation.**

|  |  |
| --- | --- |
| Description of Work: | Using a Leaf Blower (Fuel)  |
| Leaf Blower (Fuel)  Description: leaf-blowers-01 | **Potential Hazards:** Hazards associated with entanglement, impact and cutting, noise, fire and explosion and dust. |
| **Personal Protective Equipment (PPE) Required** *(Check the box for required PPE*): |
| hand protectionGloves | dust maskFace Masks | safety gogglesEyeProtection | face shieldWelding Mask | foot protectionAppropriateFootwear | hearing protHearing Protection | safety apronProtective Clothing |
| [x]  | [x]  | [x]  | [ ]  | [x]  | [x]  | [x]  |
|  **Safe Work Procedure Checklist:** |
| 1. PRE-Operation:* Wear adequate and appropriate PPE.
* Check ON/OFF switch is working prior to use.
* Check guards are fitted, secure and working.
* Check for loose/missing nuts, bolts and screws and tighten and/or replace as needed.

2. Operation:* + Ensure plant is only used where there is adequate ventilation.
	+ Do not point nozzle at people.
	+ Hold blower firmly.
	+ Minimise dust by using blower at lower speeds.
	+ Secure loose clothing.
	+ Switch off before removing or replacing the debris bag.
	+ Turn off blower prior to refuelling.
	+ Refuel only in well-ventilated area.

3. POST-Operation:* Ensure equipment is turned off before proceeding with other tasks.
* Ensure equipment is returned to storage area after use.
 |
| **Competent Persons** (The following persons are authorised to operate, supervise and test students on the equipment/process). |
| **Name:** | **Title:** | **Contact Details:** |
|  |  |  |