Safe Work Procedure

**NOTE: DO NOT use this equipment unless you have been trained in its safe use and operation**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Description of Work: | | | Operation of a Liquid Petroleum Gas (LP Gas) fuelled BBQ | | | | | | | | |
| Gas Barbeque   http://imgc.classistatic.com/cps/blnc/130129/225r1/0953i0b_20.jpeg | | | | | | **Potential Hazards:**   * Fire and explosion * Temperature * Slips/trips/falls | | | | | |
| **Personal Protective Equipment (PPE) Required** *(Check the box for required PPE*): | | | | | | | | | | | |
| hand protection Gloves | | dust mask Face Masks | | safety gogglesEyeProtection | face shield Welding Mask | | foot protection Appropriate  Footwear | | hearing prot Hearing Protection | safety apron Protective Clothing | |
|  | |  | |  |  | |  | |  |  | |
| **Safe Work Procedure Checklist:** | | | | | | | | | | | |
| 1. PRE-Operation:  LP Gas cylinders:   * Only fill LP Gas cylinders at authorised filling stations employing trained personnel * Avoid overfilling LP Gas cylinders * Ensure the LP Gas cylinder is undamaged, free of corrosion/ damaged fittings and avoid using cylinders with a test date older than ten years * Follow the connection instructions supplied with the LP Gas cylinder and avoid fitting a LP Gas cylinder to a natural gas appliance   BBQ fuelled by a LP Gas cylinder:   * Ensure a regulator is used between the LP Gas cylinder and the appliance unless the BBQ is designed for high pressure gas * Check that fittings are clean and tight -- use soapy water to check for leaks * Only use the BBQ outdoors in well ventilated and well lit areas and avoid use in high winds * Ensure a fire blanket or suitable fire extinguisher is available   2. Operation:   * Operate BBQ as per manufacturer’s instructions * Ensure that the lit BBQ is in the care of a responsible adult at all times * Never put any flammable liquid on a BBQ * Ensure adequate space is available for holding unprepared and prepared food and use appropriate BBQ implements   3. POST-Operation:   * Shut off the cylinder valve prior to disconnecting the LP Gas bottle from the BBQ * Remove all excess fat from the hot plate and drip tray once cooled. * Ensure valves are turned off firmly when not in use * Store LP Gas cylinders upright and secured on a firm level base away from any ignition source | | | | | | | | | | | |
| **Competent Persons** (The following persons are authorised to operate, supervise and test students on the equipment/process). | | | | | | | | | | |
| **Name:** | **Title:** | | | | | | | **Contact Details:** | | |
|  |  | | | | | | |  | | |