Safe Work Procedure

**NOTE: DO NOT use this machine unless you have been trained in its safe use and operation.**

|  |  |
| --- | --- |
| Description of Work: | Using an Planer (Electric) |
| electric planer | **Potential Hazards:** Mechanical and electrical hazard with the potential to cause harm through impact and cutting, and exposure to sharp objects.  |
| **Personal Protective Equipment (PPE) Required** *(Check the box for required PPE*): |
| hand protectionGloves | dust maskFace Masks | safety gogglesEyeProtection | face shieldWelding Mask | foot protectionAppropriateFootwear | hearing protHearing Protection | safety apronProtective Clothing |
| [ ]  | [ ]  | [x]  | [ ]  | [x]  | [ ]  | [x]  |
|  **Safe Work Procedure Checklist:** |
| 1. PRE-Operation/Task:* Task (e.g. Drawings, instructions, specifications etc.) is clearly understood.
* Ensure the piece of timber is well supported.
* Ensure correct height to be planed is set.
* Ensure all guarding is in place.
* Check that timber is in good condition and free from foreign materials (such as nails).
* Identify ON/OFF switch.

2. Operation/Task:* When planing the timber, ensure it done the grain of the wood.
* Keep hands clear of work piece and away from blade.

3. POST-Operation/Task:* Carefully dispose of waste material.
 |
| **Competent Person(s):** (The following persons are authorised to operate, supervise and test students on the equipment/process). |
| **Name:** | **Title:** | **Contact Details:** |
|  |  |  |