Safe Work Procedure

**NOTE: DO NOT use this machine unless you have been trained in its safe use and operation.**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Description of Work: | | | Using a Plastic Strip Heater | | | | | | | | |
| **plastics  forming heat moulder** | | | | | | **Potential Hazards:** Moving parts and electrical hazard with the potential to cause harm through exposure to projectiles, sharp objects, gases and fumes. | | | | | |
| **Personal Protective Equipment (PPE) Required** *(Check the box for required PPE*): | | | | | | | | | | | |
| hand protection Gloves | | dust mask Face Masks | | safety gogglesEyeProtection | face shield Welding Mask | | foot protection Appropriate  Footwear | | hearing prot Hearing Protection | safety apron Protective Clothing | |
|  | |  | |  |  | |  | |  |  | |
| **Safe Work Procedure Checklist:** | | | | | | | | | | | |
| 1. PRE-Operation/Task:   * Task (e.g. Drawings, instructions, specifications etc.) is clearly understood. * Ensure strip is heated to appropriate temperature (e.g. temperature controlled). * Ensure that loose clothing is restricted. * Ensure work area is appropriately ventilated. * Identify ON/OFF switch and emergency stop button (if applicable).   2. Operation/Task:   * Keep hands clear of work piece and away from strip.   3. POST-Operation/Task:   * Allow heater to cool prior to putting in storage area. | | | | | | | | | | | |
| **Competent Person(s):** (The following persons are authorised to operate, supervise and test students on the equipment/process). | | | | | | | | | | |
| **Name:** | **Title:** | | | | | | | **Contact Details:** | | |
|  |  | | | | | | |  | | |
|  |  | | | | | | |  | | |