Safe Work Procedure

**NOTE: DO NOT use this equipment unless you have been trained in its safe use and operation**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Description of Work: | | | Using a Tyre Changing Machine | | | | | | | | |
| **Tyre Changer  100_0770** | | | | | | **Potential Hazards:** Exposed moving parts with the potential to cause harm through entanglement, impact and cutting (sharp objects, crush and pinch points), electricity, ergonomics, condition, slip, trips and falls. | | | | | |
| **Personal Protective Equipment (PPE) Required** *(Check the box for required PPE*): | | | | | | | | | | | |
| hand protection Gloves | | dust mask Face Masks | | safety gogglesEyeProtection | face shield Welding Mask | | foot protection Appropriate  Footwear | | hearing prot Hearing Protection | safety apron Protective Clothing | |
|  | |  | |  |  | |  | |  |  | |
| **Safe Work Procedure Checklist:** | | | | | | | | | | | |
| 1. PRE-Operation:   * Ensure moving parts are lubricated. * Ensure operator is familiar with equipment controls. * Check equipment for damage prior to use. * Do not exceed maximum capacity stated on press. * Ensure table is clean before using. * Faulty equipment must not be used. Immediately report suspect machinery.   2. Operation:   * Never put any part of body between hydraulic ram clamps.   + Never leave the machine unattended when in operation.   + Before making adjustments, switch off and bring machine to a complete standstill.   3. POST-Operation:   * Switch off machine. * Leave the machine in a safe, clean and tidy state. | | | | | | | | | | | |
| **Competent Persons** (The following persons are authorised to operate, supervise and test students on the equipment/process). | | | | | | | | | | |
| **Name:** | **Title:** | | | | | | | **Contact Details:** | | |
|  |  | | | | | | |  | | |